AccelStepper

- Main Page
- Classes
- Files
- Examples

- Class List
- Class Members

Public Types | Public Member Functions | Protected Types | Protected Member Functions
AccelStepper Class Reference

Support for stepper motors with acceleration etc. More...

`#include <AccelStepper.h>`

List of all members.

## Public Types
enum | MotorInterfaceType { FUNCTION = 0, DRIVER = 1, FULL2WIRE = 2, FULL3WIRE = 3, FULL4WIRE = 4, HALF3WIRE = 6, HALF4WIRE = 8 }
| Symbolic names for number of pins. Use this in the pins argument the AccelStepper constructor to provide a symbolic name for the number of pins to use. More...

## Public Member Functions
| AccelStepper (uint8_t interface=AccelStepper::FULL4WIRE, uint8_t pin1=2, uint8_t pin2=3, uint8_t pin3=4, uint8_t pin4=5)
| AccelStepper (void(*forward)(), void(*backward)())
void | moveTo (long absolute)
void | move (long relative)
boolean | run ()
boolean | runSpeed ()
void | setMaxSpeed (float speed)
void | setAcceleration (float acceleration)
void | setSpeed (float speed)
float | speed ()
long | distanceToGo ()
long | targetPosition ()
long | currentPosition ()
void | setCurrentPosition (long position)
void | runToPosition ()
boolean | runSpeedToPosition ()
void | runToNewPosition (long position)
void | stop ()
void | disableOutputs ()
void | enableOutputs ()
void | setMinPulseWidth (unsigned int minWidth)
void | setEnablePin (uint8_t enablePin=0xff)
void | setPinsInverted (bool direction, bool step, bool enable=false)

## Protected Types
enum | Direction { DIRECTION_CCW = 0, DIRECTION_CW = 1 }
| Direction indicator Symbolic names for the direction the motor is turning. More...

## Protected Member Functions
void | computeNewSpeed ()
virtual void | setOutputPins (uint8_t mask)
virtual void | step (uint8_t step)
virtual void | step0 (uint8_t step)
virtual void | step1 (uint8_t step)
virtual void | step2 (uint8_t step)
virtual void | step3 (uint8_t step)
virtual void | step4 (uint8_t step)
virtual void | step6 (uint8_t step)
virtual void | step8 (uint8_t step)

## Detailed Description

Support for stepper motors with acceleration etc.

This defines a single 2 or 4 pin stepper motor, or stepper moter with fdriver chip, with optional acceleration, deceleration, absolute positioning commands etc. Multiple simultaneous steppers are supported, all moving at different speeds and accelerations.

Operation
  This module operates by computing a step time in microseconds. The step time is recomputed after each step and after speed and acceleration parameters are changed by the caller. The time of each step is recorded in microseconds. The run() function steps the motor if a new step is due. The run() function must be called frequently until the motor is in the desired position, after which time run() will do nothing.

Positioning
  Positions are specified by a signed long integer. At construction time, the current position of the motor is consider to be 0. Positive positions are clockwise from the initial position; negative positions are anticlockwise. The curent position can be altered for instance after initialization positioning.

Caveats
  This is an open loop controller: If the motor stalls or is oversped, AccelStepper will not have a correct idea of where the motor really is (since there is no feedback of the motor's real position. We only know where we think it is, relative to the initial starting point).

Performance
  The fastest motor speed that can be reliably supported is about 4000 steps per second at a clock frequency of 16 MHz on Arduino such as Uno etc. Faster processors can support faster stepping speeds. However, any speed less than that down to very slow speeds (much less than one per second) are also supported, provided the run() function is called frequently enough to step the motor whenever required for the speed set. Calling setAcceleration() is expensive, since it requires a square root to be calculated.

Examples:
  AFMotor_ConstantSpeed.pde, AFMotor_MultiStepper.pde, Blocking.pde, Bounce.pde, ConstantSpeed.pde, MultiStepper.pde, Overshoot.pde, ProportionalControl.pde, Quickstop.pde, and Random.pde.

## Member Enumeration Documentation

enum AccelStepper::Direction
| protected

Direction indicator Symbolic names for the direction the motor is turning.

Enumerator:

  DIRECTION_CCW | Clockwise.
  DIRECTION_CW | Counter-Clockwise.

enum AccelStepper::MotorInterfaceType

Symbolic names for number of pins. Use this in the pins argument the AccelStepper constructor to provide a symbolic name for the number of pins to use.

Enumerator:

  FUNCTION | Use the functional interface, implementing your own driver functions (internal use only)
  DRIVER | Stepper Driver, 2 driver pins required.
  FULL2WIRE | 2 wire stepper, 2 motor pins required
  FULL3WIRE | 3 wire stepper, such as HDD spindle, 3 motor pins required
  FULL4WIRE | 4 wire full stepper, 4 motor pins required
  HALF3WIRE | 3 wire half stepper, such as HDD spindle, 3 motor pins required
  HALF4WIRE | 4 wire half stepper, 4 motor pins required

## Constructor & Destructor Documentation

AccelStepper::AccelStepper | ( | uint8_t | interface = `AccelStepper::FULL4WIRE`,
|  | uint8_t | pin1 = `2`,
|  | uint8_t | pin2 = `3`,
|  | uint8_t | pin3 = `4`,
|  | uint8_t | pin4 = `5`
| ) |  |

Constructor. You can have multiple simultaneous steppers, all moving at different speeds and accelerations, provided you call their run() functions at frequent enough intervals. Current Position is set to 0, target position is set to 0. MaxSpeed and Acceleration default to 1.0. The motor pins will be initialised to OUTPUT mode during the constructor by a call to enableOutputs().

Parameters:

  [in] | interface | Number of pins to interface to. 1, 2, 4 or 8 are supported, but it is preferred to use the MotorInterfaceType symbolic names. AccelStepper::DRIVER (1) means a stepper driver (with Step and Direction pins). If an enable line is also needed, call setEnablePin() after construction. You may also invert the pins using setPinsInverted(). AccelStepper::FULL2WIRE (2) means a 2 wire stepper (2 pins required). AccelStepper::FULL3WIRE (3) means a 3 wire stepper, such as HDD spindle (3 pins required). AccelStepper::FULL4WIRE (4) means a 4 wire stepper (4 pins required). AccelStepper::HALF3WIRE (6) means a 3 wire half stepper, such as HDD spindle (3 pins required) AccelStepper::HALF4WIRE (8) means a 4 wire half stepper (4 pins required) Defaults to AccelStepper::FULL4WIRE (4) pins.
  [in] | pin1 | Arduino digital pin number for motor pin 1. Defaults to pin 2. For a AccelStepper::DRIVER (pins==1), this is the Step input to the driver. Low to high transition means to step)
  [in] | pin2 | Arduino digital pin number for motor pin 2. Defaults to pin 3. For a AccelStepper::DRIVER (pins==1), this is the Direction input the driver. High means forward.
  [in] | pin3 | Arduino digital pin number for motor pin 3. Defaults to pin 4.
  [in] | pin4 | Arduino digital pin number for motor pin 4. Defaults to pin 5.

References DIRECTION_CCW, and enableOutputs().

AccelStepper::AccelStepper | ( | void(*)() | forward,
|  | void(*)() | backward
| ) |  |

Alternate Constructor which will call your own functions for forward and backward steps. You can have multiple simultaneous steppers, all moving at different speeds and accelerations, provided you call their run() functions at frequent enough intervals. Current Position is set to 0, target position is set to 0. MaxSpeed and Acceleration default to 1.0. Any motor initialization should happen before hand, no pins are used or initialized.

Parameters:

  [in] | forward | void-returning procedure that will make a forward step
  [in] | backward | void-returning procedure that will make a backward step

References DIRECTION_CCW.

## Member Function Documentation

void AccelStepper::computeNewSpeed | ( |  | ) |
| protected

Forces the library to compute a new instantaneous speed and set that as the current speed. It is called by the library:

- after each step
- after change to maxSpeed through setMaxSpeed()
- after change to acceleration through setAcceleration()
- after change to target position (relative or absolute) through move() or moveTo()

References DIRECTION_CCW, DIRECTION_CW, and distanceToGo().

Referenced by moveTo(), run(), setAcceleration(), and setMaxSpeed().

long AccelStepper::currentPosition | ( |  | ) |

The currently motor position.

Returns:
  the current motor position in steps. Positive is clockwise from the 0 position.

Examples:
  Bounce.pde, MultiStepper.pde, Overshoot.pde, and Quickstop.pde.

void AccelStepper::disableOutputs | ( |  | ) |

Disable motor pin outputs by setting them all LOW Depending on the design of your electronics this may turn off the power to the motor coils, saving power. This is useful to support Arduino low power modes: disable the outputs during sleep and then reenable with enableOutputs() before stepping again.

References setOutputPins().

long AccelStepper::distanceToGo | ( |  | ) |

The distance from the current position to the target position.

Returns:
  the distance from the current position to the target position in steps. Positive is clockwise from the current position.

Examples:
  Bounce.pde, MultiStepper.pde, and Random.pde.

Referenced by computeNewSpeed(), and runToPosition().

void AccelStepper::enableOutputs | ( |  | ) |

Enable motor pin outputs by setting the motor pins to OUTPUT mode. Called automatically by the constructor.

References FULL4WIRE, and HALF4WIRE.

Referenced by AccelStepper().

void AccelStepper::move | ( | long | relative | ) |

Set the target position relative to the current position

Parameters:

  [in] | relative | The desired position relative to the current position. Negative is anticlockwise from the current position.

References moveTo().

Referenced by stop().

void AccelStepper::moveTo | ( | long | absolute | ) |

Set the target position. The run() function will try to move the motor from the current position to the target position set by the most recent call to this function. Caution: moveTo() also recalculates the speed for the next step. If you are trying to use constant speed movements, you should call setSpeed() after calling moveTo().

Parameters:

  [in] | absolute | The desired absolute position. Negative is anticlockwise from the 0 position.

Examples:
  Bounce.pde, MultiStepper.pde, Overshoot.pde, ProportionalControl.pde, Quickstop.pde, and Random.pde.

References computeNewSpeed().

Referenced by move(), and runToNewPosition().

boolean AccelStepper::run | ( |  | ) |

Poll the motor and step it if a step is due, implementing accelerations and decelerations to acheive the target position. You must call this as frequently as possible, but at least once per minimum step interval, preferably in your main loop.

Returns:
  true if the motor is at the target position.

Examples:
  Bounce.pde, MultiStepper.pde, Overshoot.pde, Quickstop.pde, and Random.pde.

References computeNewSpeed(), and runSpeed().

Referenced by runToPosition().

boolean AccelStepper::runSpeed | ( |  | ) |

Poll the motor and step it if a step is due, implmenting a constant speed as set by the most recent call to setSpeed(). You must call this as frequently as possible, but at least once per step interval,

Returns:
  true if the motor was stepped.

Examples:
  ConstantSpeed.pde.

References DIRECTION_CW, and step().

Referenced by run(), and runSpeedToPosition().

boolean AccelStepper::runSpeedToPosition | ( |  | ) |

Runs at the currently selected speed until the target position is reached Does not implement accelerations.

Returns:
  true if it stepped

Examples:
  ProportionalControl.pde.

References DIRECTION_CCW, DIRECTION_CW, and runSpeed().

void AccelStepper::runToNewPosition | ( | long | position | ) |

Moves the motor to the new target position and blocks until it is at position. Dont use this in event loops, since it blocks.

Parameters:

  [in] | position | The new target position.

Examples:
  Blocking.pde, and Overshoot.pde.

References moveTo(), and runToPosition().

void AccelStepper::runToPosition | ( |  | ) |

Moves the motor at the currently selected constant speed (forward or reverse) to the target position and blocks until it is at position. Dont use this in event loops, since it blocks.

Examples:
  Quickstop.pde.

References distanceToGo(), and run().

Referenced by runToNewPosition().

void AccelStepper::setAcceleration | ( | float | acceleration | ) |

Sets the acceleration and deceleration parameter.

Parameters:

  [in] | acceleration | The desired acceleration in steps per second per second. Must be > 0.0. This is an expensive call since it requires a square root to be calculated. Dont call more ofthen than needed

Examples:
  Blocking.pde, Bounce.pde, MultiStepper.pde, Overshoot.pde, Quickstop.pde, and Random.pde.

References computeNewSpeed().

void AccelStepper::setCurrentPosition | ( | long | position | ) |

Resets the current position of the motor, so that wherever the motor happens to be right now is considered to be the new 0 position. Useful for setting a zero position on a stepper after an initial hardware positioning move. Has the side effect of setting the current motor speed to 0.

Parameters:

  [in] | position | The position in steps of wherever the motor happens to be right now.

void AccelStepper::setEnablePin | ( | uint8_t | enablePin = `0xff` | ) |

Sets the enable pin number for stepper drivers. 0xFF indicates unused (default). Otherwise, if a pin is set, the pin will be turned on when enableOutputs() is called and switched off when disableOutputs() is called.

Parameters:

  [in] | enablePin | Arduino digital pin number for motor enable

See also:
  setPinsInverted

void AccelStepper::setMaxSpeed | ( | float | speed | ) |

Sets the maximum permitted speed. the run() function will accelerate up to the speed set by this function.

Parameters:

  [in] | speed | The desired maximum speed in steps per second. Must be > 0. Caution: Speeds that exceed the maximum speed supported by the processor may Result in non-linear accelerations and decelerations.

Examples:
  Blocking.pde, Bounce.pde, ConstantSpeed.pde, MultiStepper.pde, Overshoot.pde, ProportionalControl.pde, Quickstop.pde, and Random.pde.

References computeNewSpeed(), and speed().

void AccelStepper::setMinPulseWidth | ( | unsigned int | minWidth | ) |

Sets the minimum pulse width allowed by the stepper driver. The minimum practical pulse width is approximately 20 microseconds. Times less than 20 microseconds will usually result in 20 microseconds or so.

Parameters:

  [in] | minWidth | The minimum pulse width in microseconds.

void AccelStepper::setOutputPins | ( | uint8_t | mask | ) |
| protected virtual

Low level function to set the motor output pins bit 0 of the mask corresponds to _pin[0] bit 1 of the mask corresponds to _pin[1] You can override this to impment, for example serial chip output insted of using the output pins directly

References FULL4WIRE, and HALF4WIRE.

Referenced by disableOutputs(), step1(), step2(), step3(), step4(), step6(), and step8().

void AccelStepper::setPinsInverted | ( | bool | direction,
|  | bool | step,
|  | bool | enable = `false`
| ) |  |

Sets the inversion for stepper driver pins

Parameters:

  [in] | direction | True for inverted direction pin, false for non-inverted
  [in] | step | True for inverted step pin, false for non-inverted
  [in] | enable | True for inverted enable pin, false (default) for non-inverted

References step().

void AccelStepper::setSpeed | ( | float | speed | ) |

Sets the desired constant speed for use with runSpeed().

Parameters:

  [in] | speed | The desired constant speed in steps per second. Positive is clockwise. Speeds of more than 1000 steps per second are unreliable. Very slow speeds may be set (eg 0.00027777 for once per hour, approximately. Speed accuracy depends on the Arduino crystal. Jitter depends on how frequently you call the runSpeed() function.

Examples:
  ConstantSpeed.pde, and ProportionalControl.pde.

References DIRECTION_CCW, DIRECTION_CW, and speed().

float AccelStepper::speed | ( |  | ) |

The most recently set speed

Returns:
  the most recent speed in steps per second

Referenced by setMaxSpeed(), and setSpeed().

void AccelStepper::step | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step. Only called when a new step is required. Subclasses may override to implement new stepping interfaces. The default calls step1(), step2(), step4() or step8() depending on the number of pins defined for the stepper.

Parameters:

  [in] | step | The current step phase number (0 to 7)

References DRIVER, FULL2WIRE, FULL3WIRE, FULL4WIRE, FUNCTION, HALF3WIRE, HALF4WIRE, step0(), step1(), step2(), step3(), step4(), step6(), and step8().

Referenced by runSpeed(), and setPinsInverted().

void AccelStepper::step0 | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step using stepper functions (pins = 0) Only called when a new step is required. Calls _forward() or _backward() to perform the step

Parameters:

  [in] | step | The current step phase number (0 to 7)

Referenced by step().

void AccelStepper::step1 | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step on a stepper driver (ie where pins == 1). Only called when a new step is required. Subclasses may override to implement new stepping interfaces. The default sets or clears the outputs of Step pin1 to step, and sets the output of _pin2 to the desired direction. The Step pin (_pin1) is pulsed for 1 microsecond which is the minimum STEP pulse width for the 3967 driver.

Parameters:

  [in] | step | The current step phase number (0 to 7)

References setOutputPins().

Referenced by step().

void AccelStepper::step2 | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step on a 2 pin motor. Only called when a new step is required. Subclasses may override to implement new stepping interfaces. The default sets or clears the outputs of pin1 and pin2

Parameters:

  [in] | step | The current step phase number (0 to 7)

References setOutputPins().

Referenced by step().

void AccelStepper::step3 | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step on a 3 pin motor, such as HDD spindle. Only called when a new step is required. Subclasses may override to implement new stepping interfaces. The default sets or clears the outputs of pin1, pin2, pin3

Parameters:

  [in] | step | The current step phase number (0 to 7)

References setOutputPins().

Referenced by step().

void AccelStepper::step4 | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step on a 4 pin motor. Only called when a new step is required. Subclasses may override to implement new stepping interfaces. The default sets or clears the outputs of pin1, pin2, pin3, pin4.

Parameters:

  [in] | step | The current step phase number (0 to 7)

References setOutputPins().

Referenced by step().

void AccelStepper::step6 | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step on a 3 pin motor, such as HDD spindle. Only called when a new step is required. Subclasses may override to implement new stepping interfaces. The default sets or clears the outputs of pin1, pin2, pin3

Parameters:

  [in] | step | The current step phase number (0 to 7)

References setOutputPins().

Referenced by step().

void AccelStepper::step8 | ( | uint8_t | step | ) |
| protected virtual

Called to execute a step on a 4 pin half-steper motor. Only called when a new step is required. Subclasses may override to implement new stepping interfaces. The default sets or clears the outputs of pin1, pin2, pin3, pin4.

Parameters:

  [in] | step | The current step phase number (0 to 7)

References setOutputPins().

Referenced by step().

void AccelStepper::stop | ( |  | ) |

Sets a new target position that causes the stepper to stop as quickly as possible, using to the current speed and acceleration parameters.

Examples:
  Quickstop.pde.

References move().

long AccelStepper::targetPosition | ( |  | ) |

The most recently set target position.

Returns:
  the target position in steps. Positive is clockwise from the 0 position.

The documentation for this class was generated from the following files:

- AccelStepper.h
- AccelStepper.cpp