| MD_MAX72xx LED Matrix Arduino Library 2.4 Library to control connected MAX72XX devices as a pixel array

- Main Page
- Related Pages
- Classes
- Files

All Classes Files Functions Variables Typedefs Enumerations Enumerator Macros Pages
Generic Module

## Generic MAX7219 Modules

These modules are commonly available from many suppliers (eg, eBay) at reasonable cost. They are characterized by IN and OUT connectors at the short ends of the rectangular PCB.

Generic Module

## Module Orientation

          C  C  D  G  V
          L  S  I  N  c
          K     N  D  c
          |  |  |  |  |
          V  V  V  |  |
      D7 D6 D5 D4 D3 D2 D1 D0
    +------------------------+
    | 7  6  5  4  3  2  1  0 |- DP
    |                      1 |- A
    |                      2 |- B
    |                      3 |- C
    | O                    4 |- D
    | O  O                 5 |- E
    | O  O  O              6 |- F
    | O  O  O  O           7 |- G
    +-----+--+--+--+--+------+
          |  |  |  |  |
          V  V  V  |  |

          C  C  D  G  V
          L  S  O  N  c
          K     U  D  c
                T

## Module Interconnections

Generic modules need to be oriented with the MAX7219 IC at the top and connected using short patch cables in a spiral pattern. The display is oriented with the IC at the top.

Connecting Generic modules